 #else//This is the pin assignment of the motor board I am using.

    #define X_STEP_PIN         54
    #define X_DIR_PIN          55
    #define X_ENABLE_PIN       38
    #define X_MIN_PIN           3
    #define X_MAX_PIN           2

    #define Y_STEP_PIN         60
    #define Y_DIR_PIN          61
    #define Y_ENABLE_PIN       56
    #define Y_MIN_PIN          14
    #define Y_MAX_PIN          15

    #define Z_STEP_PIN         46
    #define Z_DIR_PIN          48
    #define Z_ENABLE_PIN       62
    #define Z_MIN_PIN          18
    #define Z_MAX_PIN          19

    #define Y2_STEP_PIN        36
    #define Y2_DIR_PIN         34
    #define Y2_ENABLE_PIN      30

    #define Z2_STEP_PIN        36
    #define Z2_DIR_PIN         34
    #define Z2_ENABLE_PIN      30

    #define E0_STEP_PIN        26
    #define E0_DIR_PIN         28
    #define E0_ENABLE_PIN      24

    #define E1_STEP_PIN        36
    #define E1_DIR_PIN         34
    #define E1_ENABLE_PIN      30

    #define SDPOWER            -1
    #define SDSS               53
    #define LED_PIN            13

  
    #define FAN_PIN            9 // (Sprinter config)
  
  #endif//ÕâÒ»¿é½áÊøÁË

  #define PS_ON_PIN          12



  #define KILL_PIN           -1



  #define HEATER_0_PIN       10   // EXTRUDER 1



  #define HEATER_1_PIN       -1


 
  #define HEATER_2_PIN       -1


  #define TEMP_0_PIN         13   // ANALOG NUMBERING
  #define TEMP_1_PIN         15   // ANALOG NUMBERING
 
 
  #define TEMP_2_PIN         -1   // ANALOG NUMBERING
  

  

  #define HEATER_BED_PIN     8    // BED



  #define TEMP_BED_PIN       14   // ANALOG NUMBERING

  #ifdef NUM_SERVOS
    #define SERVO0_PIN         11

    #if NUM_SERVOS > 1
      #define SERVO1_PIN         6
    #endif

    #if NUM_SERVOS > 2
      #define SERVO2_PIN         5
    #endif

    #if NUM_SERVOS > 3
      #define SERVO3_PIN         4
    #endif
  #endif

  #ifdef ULTRA_LCD

    #ifdef NEWPANEL
      #define LCD_PINS_RS 16
      #define LCD_PINS_ENABLE 17
      #define LCD_PINS_D4 23
      #define LCD_PINS_D5 25
      #define LCD_PINS_D6 27
      #define LCD_PINS_D7 29

      #ifdef REPRAP_DISCOUNT_SMART_CONTROLLER
        #define BEEPER 37

        #define BTN_EN1 31
        #define BTN_EN2 33
        #define BTN_ENC 35

        #define SDCARDDETECT 49
      #elif defined(LCD_I2C_PANELOLU2)
        #define BTN_EN1 47  //reverse if the encoder turns the wrong way.
        #define BTN_EN2 43
        #define BTN_ENC 32
        #define LCD_SDSS 53
        #define SDCARDDETECT -1
        #define KILL_PIN 41
      #elif defined(LCD_I2C_VIKI)
        #define BTN_EN1 22  //reverse if the encoder turns the wrong way.
        #define BTN_EN2 7
        #define BTN_ENC -1
        #define LCD_SDSS 53
        #define SDCARDDETECT 49
      #else
        //arduino pin which triggers an piezzo beeper
        #define BEEPER 33  // Beeper on AUX-4

        //buttons are directly attached using AUX-2
        #ifdef REPRAPWORLD_KEYPAD
          #define BTN_EN1 64 // encoder
          #define BTN_EN2 59 // encoder
          #define BTN_ENC 63 // enter button
          #define SHIFT_OUT 40 // shift register
          #define SHIFT_CLK 44 // shift register
          #define SHIFT_LD 42 // shift register
        #else
          #define BTN_EN1 37
          #define BTN_EN2 35
          #define BTN_ENC 31  //the click
        #endif

        #ifdef G3D_PANEL
          #define SDCARDDETECT 49
        #else
          #define SDCARDDETECT -1  // Ramps does not use this port
        #endif

      #endif

      #if MB(3DRAG)
        #define BEEPER -1

        #define LCD_PINS_RS 27
        #define LCD_PINS_ENABLE 29
        #define LCD_PINS_D4 37
        #define LCD_PINS_D5 35
        #define LCD_PINS_D6 33
        #define LCD_PINS_D7 31

       //buttons
       #define BTN_EN1 16
       #define BTN_EN2 17
       #define BTN_ENC 23 //the click

    #endif
    #else //old style panel with shift register
      //arduino pin witch triggers an piezzo beeper
      #define BEEPER 33   //No Beeper added

      //buttons are attached to a shift register
  // Not wired this yet
      //#define SHIFT_CLK 38
      //#define SHIFT_LD 42
      //#define SHIFT_OUT 40
      //#define SHIFT_EN 17

      #define LCD_PINS_RS 16
      #define LCD_PINS_ENABLE 17
      #define LCD_PINS_D4 23
      #define LCD_PINS_D5 25
      #define LCD_PINS_D6 27
      #define LCD_PINS_D7 29
    #endif
  #endif //ULTRA_LCD


// SPI for Max6675 Thermocouple

#ifndef SDSUPPORT
// these pins are defined in the SD library if building with SD support
  #define SCK_PIN          52
  #define MISO_PIN         50
  #define MOSI_PIN         51
  #define MAX6675_SS       66// Do not use pin 53 if there is even the remote possibility of using Dsplay/SD card
#else
  #define MAX6675_SS       66// Do not use pin 49 as this is tied to the switch inside the SD card socket to detect if there is an SD card present
#endif

#endif // RAMPS_OLD || RAMPS_13_EFB || RAMPS_13_EEB || RAMPS_13_EFF || 3DRAG